Quesxtions:

License?

Is ‘detector’ in NXxas deprecated and equivalent to monitor (NXmonitor)

XDI has dectector type (detector.i0, it, if, ir), which specifies how the incident flux was measured, with different values than monitor/mode.

NXxas has MonitorMode with values ‘’monitor’ or ‘timer’ for how the monitor collects counts. Seems to be the same as NEXUS ontology nxs:Field/NXmonitor/mode, but not in NXxas\_new.

Is edge energy in XDI the measured edge energy, or the pre-experiment expected edge energy? ( ie an observation or a configuration parameter?)